{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":49,"n_cols":14,"rows_kept":49,"merged":[[0,0,0,15],[1,0,1,15],[4,0,5,15],[6,0,7,15],[8,0,8,15],[9,0,23,15],[24,0,24,15],[25,0,25,6],[25,8,25,15],[26,0,26,1],[26,2,26,6],[26,10,26,15],[27,0,27,1],[27,2,27,6],[27,10,27,15],[28,0,28,1],[28,2,28,6],[28,10,28,15],[29,0,29,1],[29,2,29,6],[29,10,29,15],[30,0,30,1],[30,2,30,6],[30,10,30,15],[31,0,31,6],[31,10,31,15],[32,0,32,6],[32,10,32,15],[33,0,33,6],[33,10,33,15],[34,10,34,15],[35,2,35,6],[35,10,35,15],[36,2,36,6],[36,10,36,15],[37,2,37,6],[37,10,37,15],[38,2,38,6],[38,10,38,15],[39,0,39,1],[39,2,39,6],[39,10,39,15],[40,0,40,15],[41,0,41,15],[42,0,42,1],[42,2,42,5],[42,6,42,10],[42,11,42,12],[42,13,42,15],[43,0,43,1],[43,2,43,5],[43,6,43,10],[43,11,43,12],[43,13,43,15],[44,0,44,1],[44,2,44,5],[44,6,44,10],[44,11,44,12],[44,13,44,15],[48,0,48,15]],"flags":["formulas_cached_only"]}
[]
["    深圳市佳显电子技术有限公司                              tel:0755-29769890                             fax:0755-27315661"]
[]
[]
["JXD16032A"]
[]
[]
[]
["①PHYSICAL  DIMENSION"]
{"$rows_empty":16}
["②MECHANICAL  SPECIFICATIONS",{"$nulls":7},"③PIN  CONNECTIONS "]
["Item",null,"Nominal  Dimensions(mm)",{"$nulls":5},"Pin  ","Symbol","Function"]
["Module Size(W×H×T)",null,"122.0×44.0×13.5",{"$nulls":5},1,"VSS","Ground for Logic(GND)"]
["Viewing  Area(W×H)",null,"99.0×24.0",{"$nulls":5},2,"VDD","Power supply for Logic(+5V)"]
["Dot  Pitch(W×H)",null,"0.59×0.59",{"$nulls":5},3,"V0","Power supply for LCD Driver"]
["Dot  Size(W×H)",null,"0.55×0.55",{"$nulls":5},4,"RS","H: Data；L: Instruction Code"]
[{"$nulls":8},5,"RW","H: Read; L: Write"]
[{"$nulls":8},6,"E","Enable Signal"]
["④FEATURE",{"$nulls":7},"7~14","DB0~DB7","Data Bus Line"]
["LCD Type & Colour",null,"STN:Yellow-Green,Blue,FSTN",{"$nulls":5},15,"PSB","H:Parallel Mode;  L:Serial Mode"]
["View Angle",null,"6 O'clock",{"$nulls":5},16,"NC","NO Connect"]
["Display Type",null,"Positive Type,Negative Type",{"$nulls":5},17,"/RST","Reset Signal (Active LOW )"]
["Control IC & Package",null,"ST7920,COB",{"$nulls":5},18,"NC","NO Connect"]
["Operating Temperature",null,"-20℃～70℃",{"$nulls":5},19,"LEDA","Backlight Power(+5V)"]
["Storage Temperature",null,"-30℃～80℃",{"$nulls":5},20,"LEDK","Backlight Power(0V)"]
[]
["⑤ELECTRICAL CHARACTERISTICS (Supply current doesn't contain backlight)"]
["Item",null,"Symbol",{"$nulls":3},"Test Condition",{"$nulls":4},"Typ.",null,"Unit"]
["Operating Voltage",null,"Vdd",{"$nulls":3},"Ta=25℃",{"$nulls":4},{"v":5,"d":"5.0"},null,"V"]
["Supply Current",null,"Idd",{"$nulls":3},"Ta=25℃ , Vdd=5.0V",{"$nulls":4},1.9,null,"mA"]
[]
[]
[]
["  深圳市宝安区福永镇塘尾富华工业区第11栋3楼                                                    http://www.goodview-lcd.com"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}